VERSION "FCB V1.0"


NS_ : 
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_: MFS BCM
VAL_TABLE_ DM_ERR 1 "ERROR" 0 "NO_ERROR" ;
VAL_TABLE_ DM_KeyState 1 "PRESSED" 0 "NOT_PRESS" ;


BO_ 1008 BCM_HEAT: 8 BCM
 SG_ BCM_HEATCTL : 0|8@1+ (1,0) [0|0] ""  MFS

BO_ 1009 MFS_HOD: 8 MFS
 SG_ MFS_HOD_TEMP : 48|8@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_HOD_HEATING : 57|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_HOD_HANDING : 56|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_HOD_DIFF : 39|16@0+ (1,0) [0|0] ""  BCM
 SG_ MFS_HOD_RAW : 7|16@0+ (1,0) [0|0] ""  BCM
 SG_ MFS_HOD_baseline : 23|16@0+ (1,0) [0|0] ""  BCM

BO_ 1024 MFS_KEY: 8 MFS
 SG_ MFS_ENCODER : 48|2@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_RollDownCnt : 56|4@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_RollUpCnt : 60|4@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_SET : 12|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_RST : 11|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_DistIncrease : 14|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_DistReduce : 13|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_ADAS : 10|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_360 : 9|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_MENU : 8|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_OK : 41|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_VOICE : 43|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_RIGHT : 42|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_RETURN : 45|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_PHONE : 44|1@1+ (1,0) [0|0] ""  BCM
 SG_ MFS_KEY_LEFT : 40|1@1+ (1,0) [0|0] ""  BCM



BA_DEF_ EV_  "GenEnvIsGeneratedDsp" ENUM  "No","Yes";
BA_DEF_ EV_  "GenEnvAutoGenCtrl" ENUM  "No","Yes";
BA_DEF_ EV_  "GenEnvMsgOffset" INT 0 2147483647;
BA_DEF_ EV_  "GenEnvMsgName" STRING ;
BA_DEF_ EV_  "GenEnvIsGeneratedSnd" ENUM  "No","Yes";
BA_DEF_ SG_  "GenSigStartValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigTimeoutValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigInactiveValue" FLOAT 0 1215752192;
BA_DEF_ SG_  "GenSigMinValue" INT 0 2147483647;
BA_DEF_ SG_  "GenSigMaxValue" INT 0 2147483647;
BA_DEF_ SG_  "GenSigSendType" ENUM  "Cycle";
BA_DEF_ SG_  "GenSigEnvVarType" ENUM  "int","float","undef";
BA_DEF_ BO_  "GenMsgDelayTime" INT 0 0;
BA_DEF_ BO_  "GenMsgNrOfRepetition" INT 0 0;
BA_DEF_ BO_  "GenMsgCycleTimeFast" INT 0 0;
BA_DEF_ BO_  "NmMessage" ENUM  "No","Yes";
BA_DEF_ BO_  "GenMsgCycleTime" INT 0 65535;
BA_DEF_ BO_  "VFrameFormat" ENUM  "StandardCAN","ExtendedCAN","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","StandardCAN_FD","ExtendedCAN_FD";
BA_DEF_ BO_  "GenMsgSendType" ENUM  "Cycle";
BA_DEF_ BU_  "NmStationAddress" HEX 0 127;
BA_DEF_ BU_  "CANoeStartDelay" INT 0 0;
BA_DEF_ BU_  "CANoeDrift" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMin" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMax" INT 0 0;
BA_DEF_ BU_  "ECU" STRING ;
BA_DEF_ BU_  "NodeLayerModules" STRING ;
BA_DEF_  "BusType" STRING ;
BA_DEF_  "GenEnvVarPrefix" STRING ;
BA_DEF_  "GenEnvVarEndingSnd" STRING ;
BA_DEF_  "GenEnvVarEndingDsp" STRING ;
BA_DEF_  "DBName" STRING ;
BA_DEF_DEF_  "GenEnvIsGeneratedDsp" "No";
BA_DEF_DEF_  "GenEnvAutoGenCtrl" "No";
BA_DEF_DEF_  "GenEnvMsgOffset" 0;
BA_DEF_DEF_  "GenEnvMsgName" "";
BA_DEF_DEF_  "GenEnvIsGeneratedSnd" "No";
BA_DEF_DEF_  "GenSigStartValue" 0;
BA_DEF_DEF_  "GenSigTimeoutValue" 0;
BA_DEF_DEF_  "GenSigInactiveValue" 0;
BA_DEF_DEF_  "GenSigMinValue" 0;
BA_DEF_DEF_  "GenSigMaxValue" 0;
BA_DEF_DEF_  "GenSigSendType" "Cycle";
BA_DEF_DEF_  "GenSigEnvVarType" "undef";
BA_DEF_DEF_  "GenMsgDelayTime" 0;
BA_DEF_DEF_  "GenMsgNrOfRepetition" 0;
BA_DEF_DEF_  "GenMsgCycleTimeFast" 0;
BA_DEF_DEF_  "NmMessage" "No";
BA_DEF_DEF_  "GenMsgCycleTime" 0;
BA_DEF_DEF_  "VFrameFormat" "StandardCAN";
BA_DEF_DEF_  "GenMsgSendType" "Cycle";
BA_DEF_DEF_  "NmStationAddress" 0;
BA_DEF_DEF_  "CANoeStartDelay" 0;
BA_DEF_DEF_  "CANoeDrift" 0;
BA_DEF_DEF_  "CANoeJitterMin" 0;
BA_DEF_DEF_  "CANoeJitterMax" 0;
BA_DEF_DEF_  "ECU" "";
BA_DEF_DEF_  "NodeLayerModules" "";
BA_DEF_DEF_  "BusType" "CAN";
BA_DEF_DEF_  "GenEnvVarPrefix" "PE";
BA_DEF_DEF_  "GenEnvVarEndingSnd" "_Ps";
BA_DEF_DEF_  "GenEnvVarEndingDsp" "_Pd";
BA_DEF_DEF_  "DBName" "";
BA_ "DBName" "CanMatrix";
BA_ "NmStationAddress" BU_ BCM 1;
BA_ "GenMsgCycleTime" BO_ 1008 100;
BA_ "GenMsgCycleTime" BO_ 1009 10;
BA_ "GenMsgCycleTime" BO_ 1024 10;
VAL_ 1024 MFS_KEY_SET 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_RST 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_DistIncrease 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_DistReduce 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_ADAS 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_360 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_MENU 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_OK 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_VOICE 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_RIGHT 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_RETURN 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_PHONE 1 "PRESSED" 0 "NOT_PRESS" ;
VAL_ 1024 MFS_KEY_LEFT 1 "PRESSED" 0 "NOT_PRESS" ;

